**Figure 8. Marine mammal exclusion device “Komandor”**



Opening size: 672 x 6144 mm.

Grid mesh size before codend: 100 mm.