**Marine mammal exclusion device**

Device diagram(s): SEJONG

******

NET FOR PROTECTION OF FUR SEAL

1. P.E NET 180PLY X 300mm
2. TOP : 220 ML
3. BOTTOM : 220 ML
4. WING SIDE : 166 MD

*For each type of device used, or any change in device configuration, refer to the relevant diagram in the*

*CCAMLR fishing gear library if available (www.ccamlr.org/node/74407), or submit a detailed diagram and*

*description to the forthcoming meeting of WG-EMM.*